**T11使用说明书**

To users

Thank you for your favor with our products.

We are dedicated to providing high performance and high stability radio communication products. This two-way radio is no exception. This product is a small and exquisite walkie-talkie developed and produced by the professional team for the popularization of civil consumer market. In order to make you fully understand the various advantages of the radio performance and use and maintenance methods, please read this manual carefully.

**一 功能简介 Function Introduction**

1、3.7V Rechargeable Lithium Battery

2、Frequency Range：UHF 400-470MHZ

3、Wide/Narrow Band Selection:25KHz/12.5KHz

4、Stepped Frequency:5K/6.25K/12.5K/25K

5、Output power：2W/05W

6、50 Groups CTCSS，105 Groups DCS

7、Up to 99 Channels(1-99)

8、Time-out timer(TOT)

9、VOX Level: OFF/1/2/3/4/5

10、Busy Channel Lockout (BCLO)

11、Squelch Level:0-9

12、Battery Saving Function

13、Monitoring Function

14、Low Battery Voltage Warning/Indication

15、Chinese/English Language

16、Programmable by PC

**二 安全信息 Safety Information**

Please read the following information in order to use this two-way radio safely and efficiently.

1. The maintenance work of the two-way radio can only be carried out by professional technical personnel; assembly/dis assembly without permission is prohibited;

2. To avoid problems caused by electromagnetic interference and/or electromagnetic compatibility, please turn off the two-way radio in places with the sign “Please turn off two-way radio”, such as hospitals and other health care facilities.

3. When taking airplane, please turn off the two-way radio when the crew request.

4. In automobile with airbags, do not place the two-way radio in the inflation area of the airbags.

5. Turn off the two-way radio before entering the flammable and explosive environment;

6. Do not replace or charge the battery in flammable and explosive environments;

7. Turn off the two-way radio before approaching the blasting area and detonator area;

8. Do not use the two-way radio if the antenna is damaged, or else it may cause minor skin burns;

9. Do not expose the two-way radio to direct sunlight or near the heating device.


10. While the portable two-way radio is transmitting, keep the radio in a vertical position and keep the microphone about 5cm from the mouth.

11. Keep the two-way radio at least 2.5cm from the head or body during transmitting.

12. If you are wearing the portable two-way radio on your body, make sure that the antenna is at least 2.5cm away from the body when the two-way radio is transmitting.

13. If the two-way radio has any odor or smoke, turn off the power immediately and contact your dealer.

**三 熟悉本机**



PTT 键 PTT Button

手电灯/监听键 Flashlight/Monitor Key

LED灯 Led Lamp

信道旋钮 Channel Knob

开关/音量旋钮 Power and Volume Knob

状态指示灯Status Indicator

麦克风Microphone

LED Screens

耳机/Mac 插口 Earphone/Mac Socket

1.按键介绍 Description of the Buttons


[PTT]：When transmitting, press this button and speak to the microphone; release the button to receive.

Flashlight/Monitor Key: Press to turn on/off the flashlight; Press and hold it to turn on the monitor function.

Note:

Press and hold PTT+ "MONI" button to transmit DTMF(1750HZ, 1450HZ, 2100HZ) by default to 1750HZ，It can be set by the write frequency software (edit → optional function → DTMF).

2. LED icon and function description



1.CT（CTCSS）：When the screen displays this symbol, it represents the current channel for CTCSS receive and transmit.

2.DCS（CDCSS）：When the screen displays this symbol, it represents the current channel for CDCSS receive and transmit.

3.VOX ：When the screen displays this symbol, it represents the VOX function of the turn on.

4. (Key lock)：When the screen displays this symbol, it represents the keyboard is locked and cannot be switched up and down; except for PTT key and MONI key.

5.TX: When the screen displays this symbol, it represents is in the transmitting state, and the signal strength icon is display same time.

6.RX: When the screen displays this symbol, it represents is in the receiving state, and the signal strength icon is display same time.

7. Signal strength icon.

8. Battery level and Charging indicator：The icon represents the current battery level. When charging, the battery level jumps back and forth from 1 grid to 3 grids. (No display when power off and charging)

9. Channel number: Display current channel.

Note: The radio will enter power-saving mode after 10 seconds of standby, then the screen will be turned off, this moment, the green is flicker.

**四 功能操作 Function Operation**

1. PC 编程 Programmable by PC

The radio is connected to the computer through a special cable, which can read and write the frequency and set the function parameters etc.

1. CTCSS/CDCSS 编解码功能 CTCSS/CDCSS encode and decode

50 groups of CTCSS and 105 groups of CDCSS encode and decode functions can be set to prevent unrelated calls received on the same channel.

1. VOX 声控发射 VOX

Turn On and Off with PC programming software.

1. 繁忙禁发Busy Channel Lockout(BCLO)

To activate this function, when the channel is being used by other users, press "PTT" key, the radio will cannot transmit and "beep, beep" prompt sound.

When the channel is idle, press the "PTT" key again and it can be transmitted.

1. 超时定时器Time-out timer(TOT)

The function of the time-out timer is to prevent the any calling party from using a channel too long and continuously.

You can set this function through the programmable by PC (time:30 seconds, 60 seconds, 90 seconds, 120 seconds, 150 seconds, 180 seconds, 210 seconds, 240 seconds, 270 seconds, 300 seconds). If you continue to transmit beyond the set time, the radio will stop transmitting and beep. Release the [PTT] button and press the [PTT] button again to resume transmit.

1. 监听功能Monitor

Turn on the radio, press the “MONI” button for a long time to compulsively open the receiver and listen to whether there is any voice on the current channel.

1. 静噪电平SQL 选择Squelch Level

The frequency of squelch is 0 (on) -9 (deep), steps: 1, Level 0 is normally open SQL.

1. 自动省电功能Automatic Battery Saving Function

This function starts when the machine does not receive a signal or does not perform an operation for more than 10 seconds. The machine automatically stops this function when it receives a signal or performs an operation.

1. 语音报号功能Chinese/English voice prompts

Switch Chinese and English with PC programming software

1. 低电告警Low Battery Voltage Warning

When the battery voltage is 3.3v, the radio voice prompts: "charge battery". When the battery voltage is 3.1v, the radio is forbidden to transmit.

1. 扫描

待定。

1. 发射DTMF Transmit DTMF

Press and hold PTT+ "MONI" button to transmit DTMF(1750HZ, 1450HZ, 2100HZ) by default to 1750HZ，It can be set by the write frequency software (edit → optional function → DTMF).

**五．技术指标Technical Specification**

整体部份General

Frequency range: 400-470MHz

Memory channels: 99

Operation voltage: DC3.7V（li-ion Battery）

Frequency stability:±2.5ppm

Operation temperature: -20℃~+50℃

Mode of operation: Simplex

Antenna impedance:50Ω

Ground connection: Negative electrode

Volume: 58x28.5x172MM

Transmitter

RF Power: 2W/0.5W

Modulation: FM

Max frequency deviation:≤±5KHz

Stray Radiation:≤-60dB

Transmit current:≤1000mA

Pre-emphasis Character: 6dB/per octave

Receiver

Sensitivity: <0.16uv (12dB SINAD)

Squelch Sensitivity :< 0.2uv

Audio power:≥380mW

Audio distortion: <10%

Intermodulation: ≥65dB

Receive current: ≤380mA

Note：The above specifications/technical instructions are for reference only because of the continuous improvement of the technology. Please refer to the physical object.